5a.

We are receiving the Ascii value.

5b.

We receive 10

5c.

We receive the characters we send.

We specify the type of data we want to print by typecasting it.

6a.